**WORK INSTRUCTIONS FOR PCM ROOF AND WALKWAY CLEANING WITH HIGH PRESSURE PUMP**

# RESPONSIBILITY: PCM INCHARGE

**Identified Hazards:**

1. Fall of a person from a height
2. High pressure water discharge,
3. Electrical shock.
4. Fire & explosion
5. Dust fumes
6. Contact with lime power
7. Steaming while cleaning the PCM roof
8. Inadequate local lighting
9. Non adherence to PPE/WI
10. Improper Housekeeping

**Significant Aspect**:

1. Usage of water
2. Generation of dust
3. Generation of lime slurry

**Procedure for PCM roof and walkway cleaning:**

* Unauthorized operation or repair of any equipment is a punishable offence.
* PCM in charge should ensure that all people involved in the activity are wearing Safety shoes, helmet, safety goggles, dust mask, and hand gloves.
* PCM in charge should ensure that LOTO Lock is applied to PCM before starting the activity.
* Place the Silpaulin sheet above the moulds in order to avoid water accumulation on moulds.
* Area below the PCM under cleaning to be barricaded with work in progress tape to prevent people movement and water splashing on them and flying chips.
* PCM in charge should ensure that safety belt is used if climbing on top of PCM roof.
* PCM in charge should ensure that high pressure pump is properly used. (Refer WI/Prod/25 for High pressure pump operation.)
* Clean PCM roof, walkways, and hand railings, moulds cooling pipeline, chutes and PCM structures.
* After completion of the job, the Machine should be parked at the designated place and water hoses properly rolled.
* Machine should be parked in unplugged condition.
* Cleaning operation should be stopped if steam from cooling pigs is affecting clear vision.

|  |  |  |
| --- | --- | --- |
| **Prepared By:**  Head – Production PID I | **Reviewed & Issued By:**  Management Representative | **Approved By:**  Head – Pig Iron Division |
| **Signature:** | **Signature:** | **Signature:** |
| **Date: 15.07.2022** | **Date: 15.07.2022** | **Date: 15.07.2022** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Amendment Record** | | | |
| **Revision date** | **Manual Section ref. and para** | **Brief details of revision** | **New Revision No.** |
| 15.07.2022 | Procedure for PCM roof and walkway cleaning | Change in format | 04 |
|  |  |  |  |