**Check if described Monitoring thresholds are sufficient, valid and implemented**

Depends on the frequency we are getting alerts list out those alerts .

If threshold values are sufficient make it as completed otherwise check with Architect to modify the threshold values.