|  |  |  |  |
| --- | --- | --- | --- |
| Logo  Description automatically generated | **VEDANTA LIMITED –**  **VALUE ADDED BUSINESS** | **Format No.:** | **FRMT/MR/10** |
| **INTEGRATED MANAGEMENT SYSTEM** | **Revision Date:** | **04.04.2022** |
| **HAZARD IDENTIFICATION** | **Revision No.:** | **02** |
| **Page No.:** | **1 of 1** |

1. **Work activity information : House keeping**

|  |  |
| --- | --- |
| **Departmental Use Only** | |
| **Revision No: 03** | **Unit: Power plant 1** |
| **Revision Date: 07/08/2023** | **Dept.: MECHANICAL** |
|  |  |

|  |  |  |
| --- | --- | --- |
| **Sr.No.** | **Details** | **Remark** |
| 1) | Task being carried out, their duration and Frequency: | House keeping  Occasionally |
| 2) | Location (s) where the work is carried out. | Power plant |
| 3) | Who normally/occasionally carried out the task | Engineer on the job  Maintenance workmen on the job  Contractor workmen on job |
| 4) | Who else may be affected by the work (For example visitors, subcontractors, the public) | Production engineer  Production workmen  Visitor |
| 5) | a)Has the personnel trained for performing the task  b) Any special training required | Yes  No |
| 6) | Is the written systems of work mandatory. If yes state the procedure no. | WI/MAINT/17 |
| 7) | Is the work permit required for the task | Required when activity is carried out in gas phone area and important location. |
| 8) | Plant and machinery that may be used:  Eg : crusher, conveyor, crane, heavy earthing equipment, Truck etc, | Nil |
| 9) | Any electrically operated hand tools are used | No |
| 10) | Manufacturer’s or supplier’s instructions for operation and maintenance plant machinery and powered hand tools are available or not: | Nil |
| 11) | Chain block, tools and shackles such as wire rope, hydraulic jack etc are used. | Nil |
| 12) | What materials are handled? Size, shape, surface character and weight of materials that may be handled: | Waste items  Cylindrical/rectangular/irregular shape  Approx 250 kg max |
| 13) | Is the material is required to be moved by hand. If yes Distance and heights of the place where materials have to move by hand. | 10 kg by hand (tools & tackles)  0-50 Mt height approximately max |
| 14) | Services used Eg: compressed air, oxygen, acetylene,  LPG gas, hydraulic oil, welding electrode for welding | NO |
| 15) | Physical form of substances encountered during the work (For example fume, gas, vapor, liquid, dust/powder, solid): | Solid ,liquid |
| 16) | Content and recommendations of safety data sheets relating to substances used or encountered:  ( this is applicable in case of chemical material) | NA |
| 17) | a) Relevant acts, regulations and standards relating to the work being done, the plant and machinery used and the materials used or encountered:  b) Is the activity is reviewed for compliance to statutory requirement | Factory Act  Yes |
| 18) | What is the data (s) required to be monitored during the activity and the frequency of monitoring. | CO level in gas affected area |
| 19) | Any information available from within and outside the organization on incident, accident and ill health experience associated with the work being done, equipment and substances used: | nil |

2. From the above activity information hazards are to be identified and recorded below using Appendix 'A' of SP/41

**Hazards identified**

Mechanical Hazards: Fall of person causing injury

Electrical Hazards: Inadequate local lighting

Physical Hazards: Impact by moving machinery, Splash of oil/ grease in eye while handling

Human Behaviors: Non use of PPE (Dust Mask)

|  |  |
| --- | --- |
| **Prepared By:** Engineer– MECHANICAL – PP | **Reviewed By:** Head -Power |
| **Signature:** | **Signature:** |
| **Date: 07.08.2023** | **Date: 07.08.2023** |