|  |  |  |  |
| --- | --- | --- | --- |
| Logo  Description automatically generated | **VEDANTA LIMITED –**  **VALUE ADDED BUSINESS** | **Format No.:** | **FRMT/MR/10** |
| **INTEGRATED MANAGEMENT SYSTEM** | **Revision Date:** | **04.04.2022** |
| **HAZARD IDENTIFICATION** | **Revision No.:** | **02** |
| **Page No.:** | **1 of 1** |

**Rev No: 03** Unit: PP-1

Date: 09.04.2022 Dept: Mechanical

A. Work activity information : Boiler COFG stack bellow and top cover replacement work.

|  |  |  |
| --- | --- | --- |
| **Sr. No.** | **Details** | **Remark** |
| 1) | Task being carried out, their duration and Frequency: | Boiler COFG stack bellow and top cover replacement  Occasionally |
| 2) | Location (s) where the work is carried out. | boilers |
| 3) | Who normally/occasionally carried out the task | Contractor |
| 4) | Who else may be affected by the work (For example visitors, subcontractors, the public) | contractor |
| 5) | a) Has the personnel trained for performing the task  b) Any special training required | Yes |
| 6) | Is the written systems of work mandatory. If yes state the procedure no. | WI/MAINT/47 |
| 7) | Is the work permit required for the task | Yes |
| 8) | Plant and machinery that may be used:  Eg : crusher,  conveyor, crane, heavy earthing equipment, Truck etc, |  |
| 9) | Any electrically operated hand tools are used | Welding machine, grinding machine, 24volt hand lamp, other illumination |
| 10) | Manufacturer’s or supplier’s instructions for operation and maintenance plant machinery and powered hand tools are available or not: | Yes |
| 11) | Chain block, tools and shackles such as wire rope, hydraulic jack etc are used. | Yes and are tested |
| 12) | What materials are handled? Size, shape, surface character and weight of materials that may be handled: | Load upto-8000kg |
| 13) | Is the material is required to be moved by hand. If yes Distance and heights of the place where materials have to move by hand. | No |
| 14) | Services used Eg: compressed air, oxygen, acetylene,  LPG gas, hydraulic oil, welding electrode for welding | Oxygen,acetylene,electrode |
| 15) | Physical  form of substances encountered during the work (For example fume, gas, vapour, liquid, dust/powder, solid): | Fumes, COFG gas |
| 16) | Content and recommendations of safety data sheets relating to substances used or encountered:  ( this is applicable in case of chemical material) | nil |
| 17) | a) Relevant acts, regulations and standards relating to the work being done, the plant and machinery used and the materials used or encountered:  b) Is the activity is reviewed for compliance to statutory requirement | Checking of crane load chart before using |
| 18) | What is the data (s) required to be monitored during the activity and the frequency of monitoring. | Welding cable, cutting hose, co level at work area |
| 19) | Any information available from within and outside the organization on  incident, accident and ill health experience associated with the work being done, equipment and substances used: | Nil |

2. From the above activity information hazards are to be identified and recorded below using Appendix 'A' of SP/41

**Hazards identified**

Physical: Electric shock, high temperature gas.

Mechanical: Contact, entanglement, impact

                                 Improper house keeping

                                 Human error/human behavior

                                  Non use of PPE.

                                Alcoholism.

                                 Height phobia.

             Chemical Hazard - Fire & Explosion, Fumes, CO Gas Leakage.

|  |  |
| --- | --- |
| **Prepared By:** | **Reviewed By:** |
| **Signature:** | **Signature:** |
| **Date: 09.04.2022** | **Date: 09.04.2022** |