|  |  |  |  |
| --- | --- | --- | --- |
| A picture containing drawing  Description automatically generated | **VEDANTA LIMITED –**  **VALUE ADDED BUSINESS** | **Format No.:** | **FRMT/MR/10** |
| **INTEGRATED MANAGEMENT SYSTEM** | **Revision Date:** | **15.04.2020** |
| **HAZARD IDENTIFICATION** | **Revision No.:** | **01** |
| **Page No.:** | **1 of 1** |

**Rev No: 03** Unit: NPPL

Date: **28.05.2020**

Dept: MECHANICAL

A. Work activity information: WELDING AND CUTTING OPERATION

|  |  |  |
| --- | --- | --- |
| **Sr.No.** | **Details** | **Remark** |
| 1) | Task being carried out, their duration and Frequency: | Welding and cutting operation  1- 2 hrs  As and when reqd |
| 2) | Location (s) where the work is carried out. | Mechanical workshop/ Site |
| 3) | Who normally/occasionally carried out the task | Work men on the job  Contractor workmen taken on labor supply |
| 4) | Who else may be affected by the work (For example visitors, subcontractors, the public) | Sub contractor workmen |
| 5) | a)Has the personnel trained for performing the task  b) Any special training required | Yes (On the Job training)  No |
| 6) | Is the written systems of work mandatory. If yes state the procedure no. | WI/MAINT/NPP/31 |
| 7) | Is the work permit required for the task | Yes |
| 8) | Plant and machinery that may be used:  Eg : crusher, conveyor, crane, heavy earthing equipment, Truck etc, | Nil |
| 9) | Any electrically operated hand tools are used | Yes. Cuttoff machine |
| 10) | Manufacturer’s or supplier’s instructions for operation and maintenance plant machinery and powered hand tools are available or not: | Nil |
| **Sr.No.** | **Details** |  |
| 11) | Chain block, tools and shackles such as wire rope, hydraulic jack etc are used. | Nil |
| 12) | What materials are handled? Size, shape, surface character and weight of materials that may be handled: | Oxygen & Acetylene cylinders, Cutting set which include hoses, torch, flash back arrestor, gauges, etc. Welding cables, cutting wheels, welding rods. |
| 13) | Is the material is required to be moved by hand. If yes Distance and heights of the place where materials have to move by hand. | 1 kg by hand (consumables,tools & tackles)  2 mt height approximately |
| 14) | Services used Eg: compressed air, oxygen, acetylene,  LPG gas, hydraulic oil, welding electrode for welding | Welding electrode, oxygen, acetylene, cutting wheels |
| 15) | Physical form of substances encountered during the work (For example fume, gas, vapour, liquid, dust/powder, solid): | Solid & dust |
| 16) | Content and recommendations of safety data sheets relating to substances used or encountered:  ( this is applicable in case of chemical material) | NA |
| 17) | a) Relevant acts, regulations and standards relating to the work being done, the plant and machinery used and the materials used or encountered:  b) Is the activity is reviewed for compliance to statutory requirement | Factory Act 1948 and Goa Factory rule 1985? SRR/16  Gas Cylinder Rules 2004 SRR/14 |
| 18) | What is the data (s) required to be monitored during the activity and the frequency of monitoring. | Nil |
| 19) | Any information available from within and outside the organization on incident, accident and ill health experience associated with the work being done, equipment and substances used: | Nil |

**Hazards identified**

2. From the above activity information hazards are to be identified and recorded below using Appendix 'A' of SP/41

**Hazards identified**

Mechanical Hazard Tripping,

Fall from height,

Entangling between moving parts

Fall of spares, tools, material etc

Chemical hazard Fire & explosion, fumes

Physical Hazard Temperature, Radiation

Electrical Hazard Electrocution

Human behavior improper housekeeping, Non use of PPEs, Alcoholism, over confidence, negligence, Height phobia.

|  |  |
| --- | --- |
| **Prepared By: Abraham Mathew** | **Reviewed By: Deepak Kudalkar** |
| **Signature:** | **Signature:** |
| **Date: 28.05.2020** | **Date: 28.05.2020** |